Getting Started: Loading a precompiled demo

Selecting a device: 1

Importing a hex file: 2

Programming the device: 3

Running the device: 4

Trademarks: 4

# Selecting a device:

1) Open MPLAB® IDE

2) Select Configure->Select Device

3) Select the target device from the drop down menu

# Importing a hex file:

1) Make sure that the correct device is selected before the hex file is imported (see above for instructions).

2) Select File->Import

# Programming the device:

1) Once the correct device is selected and a hex file is imported it is ready to be programmed into a device. Select Programmer->Select Programmer->… and select the programmer that you have available and connected to the computer.

2) After the programmer is enabled connect it to the target device.

3) Select Programmer->Program to program the device.

# Running the device:

1) After the device is programmed, some programmers hold the device in reset. The easiest way to get the device running despite what programmer is being used is to disconnect the programmer from the target device.

# Trademarks:

The Microchip name and logo, the Microchip logo, MPLAB, and PIC are registered trademarks of Microchip Technology Incorporated in the U.S.A. and other countries.

PICDEM is a trademark of Microchip Technology Incorporated in the U.S.A. and other countries.

Microsoft, Windows, and Windows Vista are either registered trademarks or trademarks of Microsoft Corporation in the United States and/or other countries.